ADDRESS_ACLR_B=NONE
ADDRESS_REG_B=CLOCK1
CLOCK_ENABLE_INPUT_A=NORMAL
CLOCK_ENABLE_INPUT_B=NORMAL
CLOCK_ENABLE_OUTPUT_B=NORMAL
INTENDED_DEVICE_FAMILY="MAX 10"
LPM_TYPE=altsyncram
NUMWORDS_A=32000
NUMWORDS_B=32000
OPERATION_MODE=DUAL_PORT
OUTDATA_ACLR_B=NONE
OUTDATA_REG_B=CLOCK1
POWER_UP_UNINITIALIZED=FALSE
RAM_BLOCK_TYPE=M9K
WIDTHAD_A=15
WIDTHAD_B=15
WIDTH_A=10
WIDTH_B=10
WIDTH_BYTEENA_A=1
DEVICE_FAMILY="MAX 10"
address_a
address_b
clock0
clock1
clocken0
clocken1
data_a
wren_a
q_b
